DYNATRON/BONDO CORPORATION -- # 604 TAN POLISHING COMPOUNDS -- 7930-00N018486

===================== Product Identification =====================

Product ID:# 604 TAN POLISHING COMPOUNDS

MSDS Date:10/22/1988

FSC:7930

NIIN:00N018486

MSDS Number: BLFRD

=== Responsible Party ===

Company Name:DYNATRON/BONDO CORPORATION

Address:3700 ATLANTA INDUSTRIAL PARKWAY NW

City:ATLANTA

State:GA

ZIP:30331-1098

Country:US

Info Phone Num:800-241-3386

Emergency Phone Num:404-696-2730 404-971-1502

CAGE:16522

=== Contractor Identification ===

Company Name:BONDO/MAR-HYDE CORP

Address:3700 ATLANTA INDUSTRIAL PKWY NW

Box:City:ATLANTA

State:GA

ZIP:30331

Country:US

Phone:404-696-2730

CAGE:16522

============= Composition/Information on Ingredients =============

Ingred Name:WATER BASE COMPOUND CONTAINING INGREDIENTS 2, 3, AND 4.

RTECS #:9999999ZZ

Fraction by Wt: > 50%

Ingred Name:KEROSENE

CAS:8008-20-6

RTECS #:OA5500000

Ingred Name:TALL OIL (STRAIGHT CHAIN FATTY ACID)

CAS:61790-12-3

Ingred Name:TERPINEOL

CAS:8006-39-1

RTECS #:WZ6600000

Ingred Name:SILICA, CRYSTALLINE - TRIPOLI

CAS:1317-95-9

RTECS #:VV7336000

Fraction by Wt: < 50%

OSHA PEL:SEE TABLE Z3

ACGIH TLV:0.1 MG/M3 RDUST;9293

===================== Hazards Identification =====================

LD50 LC50 Mixture:NONE SPECIFIED BY MANUFACTURER.

Routes of Entry: Inhalation:YES Skin:YES Ingestion:NO

Reports of Carcinogenicity:NTP:NO IARC:YES OSHA:NO

Health Hazards Acute and Chronic:ACUTE: PROLONGED EXPOSURE MAY CAUSE

IRRITATION IN EYES, NOSE, MOUTH, THROAT AND ON THE SKIN. CHRONIC:

CHRONIC HUMAN HEALTH EFFECTS WOULD NOT BE EXPECTED AS LONG AS GOOD

PERSONAL HYDIENE AND PROPER SAF ETY PRECAUTIONS ARE PRACTICED.

Explanation of Carcinogenicity:CRYSTALLINE SILICA: CLASS 2A (IARC)

Effects of Overexposure:SEE HEALTH HAZARDS.

Medical Cond Aggravated by Exposure:NONE KNOWN.

======================= First Aid Measures =======================

First Aid:EYES: FLUSH WITH PLENTY OF WATER FOR AT LEAST 15 MIN. IF

IRRITATION OCCURS, CALL A PHYSICIAN. SKIN: WASH WITH SOAP AND

WATER. IF IRRITATION OCCURS, CALL A PHYSICIAN. INHAL: REMOVE TO

FRESH AIR. REST I N HALF UPRIGHT POSITION. SEEK MEDICAL ATTENTION

IF NECESSARY. INGEST: DO NOT INDUCE VOMITING. CONTACT A PHYSICIAN.

===================== Fire Fighting Measures =====================

Flash Point Method:CC

Flash Point:>125F,>52C

Lower Limits:0.7 %

Upper Limits:5.0 %

Extinguishing Media:CO2, FOAM OR DRY CHEMICAL.

Fire Fighting Procedures:AVOID USE OF WATER STREAM. WATER MAY BE USED

TO COOL FIRE EXPOSED CONTAINERS. WEAR NIOSH/MSHA APPROVED SCBA AND

FULL PROTECTIVE EQUIPMENT .

Unusual Fire/Explosion Hazard:NONE.

================== Accidental Release Measures ==================

Spill Release Procedures:REMOVE ALL SOURCES OF IGNITION FROM THE AREA.

SWEEP UP WITH INERT ABSORBER AND WASH AREA WITH WATER. AVOID

RELEASE INTO DRAINS AND WATERWAYS.

Neutralizing Agent:NONE SPECIFIED BY MANUFACTURER.

====================== Handling and Storage ======================

Handling and Storage Precautions:KEEP AWAY FROM OEPN FLAMES AND

EXCESSIVE HEAT.

Other Precautions:WARNING! PRODUCT MAY CONTAIN TRACE AMOUNTS OF SOME

CHEMICALS CONSIDERED BY THE STATE OF CALIFORNIA TO BE CARCINOGENS

OR REPRODUCTIVE TOXICANTS. (CALIF PROP 65 REPORTABLE)

============= Exposure Controls/Personal Protection =============

Respiratory Protection:AVOID BREATHING OF VAPROS. USE ADEQUATE

VENTILATION. IF USING THIS COMPOUND REQUIRES RUBBING, GRINDING OR

MACHINE POLISHING, USE NIOSH/MSHA APPROVED DUST MASK OR OSHA

APPROVED RESPIRATOR WITH DUST FIL TER.

Ventilation:LOCAL OR GENERAL EXHAUST.

Protective Gloves:NEOPRENE, NITRILE, OR POLYVINYL ALCOHOL.

Eye Protection:CHEMICAL WORKERS GOGGLES .

Other Protective Equipment:NONE SPECIFIED BY MANUFACTURER.

Work Hygienic Practices:CLEAN HANDS WITH SOAP AND WATER AFTER EVERY

USAGE.

Supplemental Safety and Health

NONE SPECIFIED BY MANUFACTURER.

================== Physical/Chemical Properties ==================

HCC:F4

Boiling Pt:B.P. Text:376F,191C

Vapor Pres:0.01 @ 68F

Vapor Density:8.0

Spec Gravity:1.25

Solubility in Water:SLIGHT

Appearance and Odor:TAN/KEROSENE ODOR.

Percent Volatiles by Volume:< 25

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

STRONG OXIDIZERS AND ALKALIES.

Stability Condition to Avoid:HEAT, SPARKS AND OPEN FLAMES.

Hazardous Decomposition Products:CARBON MONOXIDE, ALDEHYDES, AROMATICS

AND OTHER HYDROCARBONS.

==================== Disposal Considerations ====================

Waste Disposal Methods:DISPOSE IN ACCORDANCE WITH FEDERAL, STATE, AND

LOCAL REGULATIONS.

Disclaimer (provided with this information by the compiling agencies):

This information is formulated for use by elements of the Department

of Defense. The United States of America in no manner whatsoever,

expressly or implied, warrants this information to be accurate and

disclaims all liability for its use. Any person utilizing this

document should seek competent professional advice to verify and

assume responsibility for the suitability of this information to their

particular situation.